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I. Network partition

Description of event: a high level switch or major cable fails, causing a portion of the compute nodes to be inaccessible from the rest of the nodes for an unknown period of time.

Desired notification policy options:

Notification of failure

1. All processes are preemptively notified of failure before they try to communicate with processes in another partition.

2. Process only notified when it tries to communicate with node in another partition.

Notification of repair

1. Application never notified of repair that fixes the network partition. Application responsible for ensuring that different partitions don’t interfere with each other.
2. All processes are notified when partition is repaired.

3. Application must explicitly designate a process to be informed of the repair and is only notified if it has done so.
II. Link Failure
Description of event: The failure of a network link or low-level switch prevents a subset of processes from communicating with another subset. For example, in a statically-routed torus topology the failure of one or more key links or nodes can prevent a specific pair of nodes from communicating while leaving other nodes free to communicate with each other.

Desired notification policy options:

Notification of failure (processes A and B can’t communicate with each other)

1. Processes A and B preemptively notified of failure before they try to communicate with each other.

2. When process A tries to communicate with B or vice versa, it is informed of failure.

3. When process C tries to perform a collective operation that involves both A and B, it is informed of the failure.

Notification of repair

1. Both A and B notified when connection between them is repaired.

2. Application must explicitly designate a process to be informed of the repair and is only notified if it has done so.

III. Global or local network performance degradation
Description of event: performance is degraded because 
· (global) Some replicated high-level switches have failed causing all cross-machine communication to pass through fewer switches.

· (global) The network is being shared with another application, which has entered a communication-heavy phase.
· (local) Some replicated low-level switches have failed causing all local communication to pass through fewer switches.

· (local) A given network wire has become frayed, causing its re-transmit rate to increase significantly. 

Desired notification policy options:

Notification of degradation

1. All affected processes are informed before their next communication operation.

2. Each affected process informed at the time of its next communication operation.

3. Each process that participates in a collective call with an affected process is informed at the time of the call.

4. Application must explicitly designate a process to be informed of the degradation and is only notified if it has done so.

Notification of repair

1. All affected processes are informed before their next communication operation.

2. Each affected process informed at the time of its next communication operation.

3. Application must explicitly designate a process to be informed of the repair and is only notified if it has done so.
